Cobertura CHRYSLER en versión PKG50

Linea de datos hasta 2006-2009 con gráficas y autodetección.

Sistemas:
ENGINE PCM
ABS
AUTOMATIC SWAY BAR SYSTEM
AIRBAG
SAS STEERING WHEEL ANGLE
WCM O SKREEM O SKIM O ANTENA
AMPLIFIER

TIPM MODULO DE ALIMENTACION DE CORRIENTE
INTEGRATED POWER MODULE

ENGINE PCM

CURRENT FUEL SHUTOFF
SKIM VTA KEY RECEIVED FAULT
NGC SHOWLD SHUT OFF FUEL
SKIM /VTA HAS COMPLETED
MAP VACUM
MAP VOLTS
BARO PRESSURE
ACCELERATOR PEDAL POSITION
APP 1 VOLT
APP2 VOLT
TPS MIN VOLTS
TPS 1 VOLTS
TPS 2 MIN VOLTS
TPS 2 VOLTS
THROTTLE BLADE POSITION
ETC DIRECTIONAL DUTY CYCLE
ENGINE SPEED
TARGET IDLE SPEED
TIME FROM START RUN
TIME FUEL SYSTEM IN RUN MODE
IGNITION OFF TIME
ENGINE RUNTIME
PURGE DUTY CYCLE
DESIRED PURGE CURRENT
ACTUAL PURGE CURRENT
PURGE AIRFLOW
PURGE MODE
PURGE VAPOR RATIO
PURGE ADAPTIVE
DESIRED DOUBLE START OVERIDE
ACTUAL TORQUE
ETC STARTER INHIBIT
EGR SENSOR VOLTS
EGR DUTY CYCLE
EGR FLOW
DESIRED EGR POSITION
ACTUAL EGR POSITION
INJECTOR PULSE WIDTH CYL 1
INJECTOR PULSE WIDTH CYL 2
INJECTOR PULSE WIDTH CYL 3
INJECTOR PULSE WIDTH CYL 4
INJECTOR PULSE WIDTH CYL 5
INJECTOR PULSE WIDTH CYL 6
CRANKING INJECTOR PULSE WIDTH
1/1 O2 SENSOR LEVEL
2/1 O2 SENSOR LEVEL
1/1 O2 GOAL (0-1)
2/1 O2 GOAL (0-1)
1/1 O2 VOLTS (0-1)
1/1 O2 SENSOR VOLTS
1/2 O2 VOLTS (0-1)
1/2 O2 SENSOR VOLTS
2/1 O2 VOLTS (0-1)
2/1 O2 SENSOR VOLTS
2/2 O2 VOLTS (0-1)
2/2 O2 SENSOR VOLTS
1/1 O2 FUEL FEEDBACK
2/1 O2 FUEL FEEDBACK
1/1 PULSE WIDTH O2 HEATER
1/2 PULSE WIDTH O2 HEATER
2/1 PULSE WIDTH O2 HEATER
2/2 PULSE WIDTH O2 HEATER
1/1 O2 HEATER TEMP
1/2 O2 HEATER TEMP
2/1 O2 HEATER TEMP
2/2 O2 HEATER TEMP
1/1 SHORT TERM ADAP
2/1 SHORT TERM ADAP
1/1 LONG TERM ADAP
2/1 LONG TERM ADAP
CLOSED LOOP TIMER
CURRENT ADAP CELL ID
ENGINE COOLANT TEMP
ENGINE COOLANT TEMP VOLT
INTAKE AIR TEMP DEG
INTAKE AIR TEMP VOLT
AMBIENT TEMP
FUEL LEVEL PERCENT
FUEL TANK VAPOR VOLUME
FUEL TANK SIZE
FUEL LEVEL SENSOR #1 VOLTS
AMBIENT TEMP VOLTAGE
CAT MODELED TEMP
OIL PRESS SW
VOLTAGE SENSE
TARGET CHARGING VOLTAGE
GENERATOR DUTY CYCLE
MASS AIRFLOW
KNOCK SENSOR 1 VOLTS
ST KNOCK RETARD
BASE SPARK
SPARK ADVANCE
ESIM SWITCH
AC HI-SIDE PRESSURE
AC HI-SIDE VOLTAGE
PCM ODOMETER
VEHICLE SPEED
CAM SYNC STATE
CRANK SIGNAL MISSING
CRANK SYNC STATE
CRANK SYSTEM FAULT AND IN LIMP-HOME MODE
CAM CRANK DIFFERENCE
BRAKE SW FILTERED SW STATE
BRAKE SW 2 FILTERED SW STATE
PARK NEUTRAL SW FILTERED SW STATE
AC SELECT SW FILTERED SW STATE
AC REQUEST SW FILTERED SW STATE
ACT A/C CLUTCH RELAY
AC OUTPUT CURRENT
DESIRED LOW SPEED FAN
DESIRED HIGH SPEED FAN
ASD SENSE SW FILTERED SW STATE
DESIRED ASD RELAY
FUEL PUMP RELAY
IGN START SW FILTERED SW STATE
DESIRED MALFUNCTION LAMP
S/C SW VOLTAGE
S/C SW VOLTAGE 2
CRUISE LAMP STATUS
S/C WORKING STATUS
S/C DENIED STATUS
S/C DISENABLE REASON
S/C DISENGAGE REASON
S/C SW STATE 1
S/C SW STATE 2

LINEA DE DATOS DE ABS
VALVE FEED
POWER SUPPLY VOLTAGE
ABS PUMP FEED
LF WHEEL SPEED
RF WHEEL SPEED
RR WHEEL SPEED
RL WHEEL SPEED
PRESSURE SENSOR
LONGITUDINAL SENSOR
YAW SENSOR
STEERING ANGLE SENSOR POSITION
LATERAL ACCELERATION
IGNITION SENSE
VEHICLE SPEED
LF WHEEL SPEED
RF WHEEL SPEED
RR WHEEL SPEED
RL WHEEL SPEED
BRAKE PEDAL STATUS
LINEA DE DATOS DE ASBS O AUTOMATIC SWAY BAR SYSTEM (DIRECCION)
IGNITION STATUS
IGNITION OFF TIME
ASBS MECHANICAL BRAKE STATUS
SMARTBAR STATE
SMARTBAR REDISENGAGE SPEED THRESHOLD
SMARTBAR DISENGAGE SPEED THRESHOLD
FORK POSITION AVERAGE
FORK TRAVEL
PLUNGER TRAVEL
TRANSFER CASE STATUS
PLUNGER POSITION TOOTH COUNT
MOTOR MINIMUM DUTY CYCLE
LINEA DE DATOS DE AIRBAG ORC
ECU VOLTAGE SOURCE
IGNITION VOLTAGE
AIRBAG LAMP (SRS INDICATOR)
PASSENGER AIRBAG DISABLE LAMP
VEHICLE IS EQUIPED WITH SIDE AIRBAG
SYSTEM VOLTAGE
PASSENGER AIRBAG DISABLE SW PRESENT
VEHICLE SPEED
ENGINE SPEED
IGNITION SWITCH STATUS
LINEA DE DATOS DE SAS STEERING WHEEL ANGLE
SAS NOT INITIALIZED
BOTH PROCESSORS HAVE DIFF RESULTS
STEERING WHEEL ANGLE SENSOR STATUS
STEERING WHEEL ANGLE
LINEA DE DATOS DE WCM O SKREEM O SKIM O ANTENA
ECU STATUS
IGNITION VOLTAGE
IGNITION STATUS
IGNITION SW VOLTAGE VALUE
NUMBER OF KEY/FOBS PROGRAMMED
KEY FOB ID (DEPRESSED)
RKE FOB BUTTON DEPRESSED
LAST KEY FOB ID DEPRESSED
KEYFOB BUTTON DEPRESSED
KEY FOB BUTTON STUCK
LAST KEY FOB ID W/STUCK BUTTON
IGNITION CYCLE COUNTER
SENSOR 1 IDENTIFICATION
SENSOR 2 IDENTIFICATION
SENSOR 3 IDENTIFICATION
SENSOR 4 IDENTIFICATION
SENSOR 5 IDENTIFICATION
TIRE PLACARD PRESSURE - FRONT
TIRE PLACARD PRESSURE - REAR
TIRE LOW PRESSURE THRESHOLD - FRONT
TIRE LOW PRESSURE THRESHOLD - REAR
LOW PRESSURE THRESHOLD HYSTERESIS
TIRE 1 PRESSURE SENSOR HW FAULT
TIRE 1 PRESSURE SENSOR HW OVERFLOW/UNDERFLOW
TIRE 1 TEMPERATURE SENSOR HW FAULT
TIRE 1 TEMPERATURE SENSOR HW OVRFLOW/UNDERFLOW
TIRE 1 ACCELERATION SENSOR HW FAULT
TIRE 1 ACCELERATION SENSOR HW OVERFLOW/UNDERFLOW
TIRE 2 PRESSURE SENSOR HW FAULT
TIRE 2 PRESSURE SENSOR HW OVERFLOW/UNDERFLOW
TIRE 2 TEMPERATURE SENSOR HW FAULT
TIRE 2 TEMPERATURE SENSOR HW OVRFLOW/UNDERFLOW
TIRE 2 ACCELERATION SENSOR HW FAULT
TIRE 2 ACCELERATION SENSOR HW OVERFLOW/UNDERFLOW
TIRE 3 PRESSURE SENSOR HW FAULT
TIRE 3 PRESSURE SENSOR HW OVERFLOW/UNDERFLOW
TIRE 3 TEMPERATURE SENSOR HW FAULT
TIRE 3 TEMPERATURE SENSOR HW OVRFLOW/UNDERFLOW
TIRE 3 ACCELERATION SENSOR HW FAULT
TIRE 3 ACCELERATION SENSOR HW OVERFLOW/UNDERFLOW
TIRE 4 PRESSURE SENSOR HW FAULT
TIRE 4 PRESSURE SENSOR HW OVERFLOW/UNDERFLOW
TIRE 4 TEMPERATURE SENSOR HW FAULT
TIRE 4 TEMPERATURE SENSOR HW OVRFLOW/UNDERFLOW
TIRE 4 ACCELERATION SENSOR HW FAULT
TIRE 4 ACCELERATION SENSOR HW OVERFLOW/UNDERFLOW
TIRE 5 PRESSURE SENSOR HW FAULT
TIRE 5 PRESSURE SENSOR HW OVERFLOW/UNDERFLOW
TIRE 5 TEMPERATURE SENSOR HW FAULT
TIRE 5 TEMPERATURE SENSOR HW OVRFLOW/UNDERFLOW
TIRE 5 ACCELERATION SENSOR HW FAULT
TIRE 5 ACCELERATION SENSOR HW OVERFLOW/UNDERFLOW
TMP LOCALIZATION FAULT
DUPLICATE TPM SENSOR IDS
MISSING TPM SENSOR IDS
SENSOR IN SLEEP MODE
BUSSED INPUTS
ENGINE SPEED
NGC/SKREEM STATUS
IGNITION STATUS
ENGINE RESET NOTIFICATION
BUSSED OUTPUTS
KEY IN IGNITION
SKIM KEY NUMBER IGNITION
VALID SKIM KEY
SKREEM SEED REQUEST TO ENGINE
SKREEM STATUS
RKE FOB NUMBER REQUEST
RKE BASIC FUNCTION REQUEST
RKE COMPLEX FUNCTION REQUEST
PANIC MODE
SKREEM CHIME REQUEST
TPM CHIME REQUEST
INDICATOR LAMP STATUS
TIRE PRESSURE INDICATOR REQUEST
TPM SYSTEM LOCALIZATION STATUS
LINEA DE DATOS DE AMPLIFIER
BATTERY VOLTAGE
CABIN EQUALIZATION CURVE NUMBER
SYSTEM VOLTAGE
IOD FUSE STATUS
ACCESSORY DELAY IS ACTIVE
AMP MUTE STATUS
LINEA DE DATOS DE INSTURMENTOS O CNN O INSTRUMENT CLUSTER
IOD POWER
IGNITION RUN/START
AC EVAP SENSOR VOLTAGE
HVAC SWITCH VOLTAGE
EVAP SENSOR TEMPERATURE
HVAC SWITCH POSITION
BRAKE SWITCH
EBL SWITCH
HARD TOP STATUS
PARKING BRAKE SWITCH
ESP/TRAC OFF SWITCH
COURTESY LAMPS
4WD SWITCH STATUS
CONVENIENCE LIGHTING
BTSI CONTROL
UGDO CONTROL
A/C LED
EBL LED
TOW MODE (O/D OFF) SWITCH
A/C SELECT LED
HORN SWITCH
INTERIOR LIGHTING DIMMER SW VOLTAGE
4WD SWITCH VOLTAGE
INTERIOR LIGHTING DIMMER SW
EXTERIOR LIGHTING SW STATUS
EXTERIOR LIGHTING SW VOLTAGE
BUSSED INPUTS
COMMANDED IGNITION SWITCH STATUS
IGN RUN ACTIVE FOR REMOTE START
LOW BRAKE FLUID WARNING
ENGINE COOLANT LEVEL LOW
THROTTLE PEDAL POSITION (CALCULATED)
ENGINE SPEED
VEHICLE SPEED
AUTOMATIC OIL CHANGE INDICATOR
LOW WASHER FLUID WARNING
PASSENGER DOOR AJAR
DRIVER DOOR AJAR
FLIPPER GLASS AJAR
TRANSFER CASE CLUSTER DISPLAY
CRUISE ON
REVERSE GEAR
SYSTEM VOLTAGE
PARKLAMPS ARE ON
RIGHT TURN SIGNAL ON
LEFT TURN SIGNAL ON
LOW BEAM IS ON
FRONT FOG IS ON
HIGH BEAM IS ON
FUEL LEVEL 2 A/D VOLTAGE
AMBIENT TEMPERATURE
FUEL LEVEL A/D VOLTAGE
AUTO WIPER CONFIGURATION
SOUND HORN ON LOCK
LOAD SHEDDING LEVELS
SMART ACCESSORY DELAY IS ACTIVE
AUTO LOCK
DOOR ALERT
AUTO UNLOCK
FLASH LAMPS WITH LOCK
CHIME REQUEST
POWER ACCESORY DELAY TIME
HEADLAMP DELAY TIME
UNLOCK ALL DOORS ON 1ST PRESS
HEADLAMPS ON WITH WIPER
ILLIMINATED APPROACH TIME
RIGHT REAR TURN SIGNAL FAILURE
RIGHT FRONT TURN SIGNAL FAILURE
LEFT FRONT TURN SIGNAL FAILURE
LEFT REAR TURN SIGNAL FAILURE
SWAY BAR INDICATOR REQUEST
REQUEST MIL BLINK
DRIVING PROGRAM DISPLAY CODE
ETC FAULTY, INDICATOR LAMP REQUEST
BRAKE ASSIST FAULTY
ESP INDICATOR LAMP, STEADT STATE
ESP INDICATOR LAMP, FLASHING LIGHT REQ
ESP FAULTY. INDICATOR LAMP REQ
REQUEST MIL ON
ABS FAULTY
REQUEST OIL LEVEL/OIL PRESSURE INDICATOR LAMP
PRNDL DISPLAY REQ
CRUISE ENGAGED
CHARGING SYSTEM FAILURE
ELECTRONIC THROTTLE CONTROL
BUSSED OUTPUTS
ODOMETER
AVERAGED AMBIENT TEMP
HORN REQUEST
OPTIAL HORN REQ
AC EVAPORATOR TEMP
EVAPORATOR TEMP TARGET
OVERDRIVE SWITCH PRESSED
LANGUAGE CHANGE REQUEST
US OR METRIC
FRONT SWAYBAR CONTROL SWITCH STATUS
AXLE LOCK SW STATUS
ELECTRIC BACKLIGHT STATUS
A/C REQUEST
PTC HEATER ENABLE
DISABLE REAR PTC
DISABLE HEV AUTOSTOP
A/C SELECT
DEFROST SELECT SW
LEFT AMBIENT LIGHT SENSOR
LIN
DIM SWITCH SETTING
TRACTION CONTROL /ESP PRESSED
PADL LAMP STATUS
INVERTER REQUEST
ELECTRIC BACKLIGHT REQ
WALKEUP REASON FOR ASBM
RESPONSE ERROR ASBM
HAZARD REQ
AXLE LOCK SW STATUS
FOG LAMP REQ
REAR WIPER WASH REQ ON
WAKE UP REASON FOR MFS
HEAD LAMP REQ
OPTICAL HORN REQ ON
REAR WIPER REQ ON
RESPONSE ERROR MFS
HIGH BEAM ON REQUEST
TURN SIGNAL REQUEST
FRONT WIPER INTERVAL SETTING SW
FRONT WIPER WASH REQ
FRONT MIST WIPER REQ ON
DISTORTION DETECTED
COMPASS (NSEW)
SENSOR FAULT
CALIBRATION FAULT
NVM FAULT
COMPASS (DEGREES)
VARIANCE VALUE
CALIBRATION MODE
RCM FAULT
CALIBRATION REQUIRED
FRONT SWAYBAR CONTROL SWITCH STATUS
LINEA DE DATOS DE AMPLIFIER
VEHICLE ENTRETAINMENT SYSTEM (VES)
HANDS FREE MODULE (HFS)
DISP
VES2
AM/FM SIGNAL STRENGHT
LW
AM/MW
FM
AUDIO PLAYING IN FL SPEAKER QUADRANT
AUDIO PLAYING IN FR SPEAKER QUADRANT
AUDIO PLAYING IN RL SPEAKER QUADRANT
AUDIO PLAYING IN RR SPEAKER QUADRANT
RADIO VOLUME SETTING
BASS SETTING
TREBLE SETTING
BALANCE SETTING
FADE SETTING
MID-RANGE SETTING
BUSSED INPUTS
IGN SW STATUS
ACCESORY DELAY IS ACTIVE
REAR CAMERA PRESENT
PROGRAM UP/DOWN
REMOTE STEERING WHEEL SW
AUDIO SYSTEM MUTE REQ FROM PTS
DVD REGION CODE
RADIO MARKET SELECT
CLOCK DISPLAY
REMOVABLE HARD TOP IS OFF
CONVERTIBLE TOP SW REQ
CONVERTIBLE TOP STATUS
LANGUAGE PREFERENCE
BUSSED OUTPUTS
DISWC IN LOADED IN 1
DISWC IN LOADED IN 2
DISWC IN LOADED IN 3
DISWC IN LOADED IN 4
DISWC IN LOADED IN 5
DISWC IN LOADED IN 6
LANGUAGE CHANGE REQ FROM RADIO
AUDIO LEVEL
LINEA DE DATOS DE TIPM MODULO DE ALIMENTACION DE CORRIENTE INTEGRATED POWER MODULE
AMBIENT TEMP DEG
AMBIENT TEMP VOLT
AC REFRIGERANT PRESS
AC REFRIGERANT VOLTAGE
A/C CLUTCH SENSE
RADIATOR FAN 1 DUTY CYCLE
RADIATOR FAN 2 DUTY CYCLE
IOD SENSE
SWITCHED BATTERY VOLTAGE 1
SWITCHED BATTERY VOLTAGE 2
SWITCHED BATTERY VOLTAGE 3
IGNITION SW STATUS
IGNITION RUN/START SENSE
BATTERY VOLTAGE
FRONT WIPER PARK SW SENSE
REAR WIPER PARK SIGNAL
WASHER MOTOR STATE
WASHER FLUID LEVEL VOLTAGE
WASHER FLUID LEVEL
HAZARD SW
RIGHT FRONT DOOR AJAR SW
RIGHT FRONT SW VOLTAGE
RIGHT FRONT DOOR SW
LEFT FRONT DOOR AJAR SW
LEFT FRONT DOOR SW VOLTAGE
LEFT FRONT DOOR SW
OUTSIDE HANDLE SW VOLTAGE
OUTSIDE HANDLE SW
LEFT REAR DOOR AJAR SW
RIGHT REAR DOOR AJAR SW
BRAKE FLUID LEVEL VOLTAGE
BRAKE FLUID LEVEL VOLTAGE
BRAKE FLUID LEVEL
BRAKE SW SENSE
FUEL LEVEL SENSE 1
FUEL LEVEL SENSE 2
LEFT LOW BEAM DUTY CYCLE
RIGHT LOW BEAM DUTY CYCLE
LEFT HIGH BEAM DUTY CYCLE
RIGHT HIGH BEAM DUTY CYCLE
REVERSE GEAR SW
T-CASE ENCODER SENSOR
T-CASE ENCODER SENSOR VOLTAGE
FRONT AXLE LOCK FEEDBACK SIGNAL
REAR AXLE LOCK FEEDBACK SIGNAL
FRONT AXLE LOCK ENABLE
REAR AXLE LOCK ENABLE
WHEEL SPEED SENSOR
LOW COOLANT LEVEL
LIFTGATE OR TRUNK AJAR SW
LEFT FRONT SEATBELT BUCKE SW
LEFT FRONT TURN LAMP
RIGHT FRONT TURN LAMP
INVERTER CONTROL RELAY DRIVER
5 VOLT SENSOR SUPPLY
THATCHUM UN-LOCK MOTOR RELAY COIL
THATCHUM UN-LOCK MOTOR RELAY COIL
SWAY BAR COIL DRIVER ENABLE #1
SWAY BAR COIL DRIVER ENABLE #2
DIESEL COIL ·1 CONTROL - GLOW PLUG
DIESEL COIL ·2 CONTROL - GLOW PLUG
LEFT FRONT DOOR UNLOCK
PASSENGER DOORS UNLOCK
ALL DOORS LOCK
LEFT LOW BEAM/HID
FRONT WIPER LOW
REAR WIPER
IGN RUN/START 1
IGN RUN 1
IGN RUN/ACC 1
LEFT FRONT FOG LAMPS
RIGHT FRONT FOG LAMPS
AC CLUTCH
FRONT WIPER HIGH
REVERSE LAMPS
RIGHT LOW BEAM/HID
BLOWER MOTOR
LEFT HIGH BEAM
DEFROST (MIRROR/EBL)
RIGHT HIGH BEAM
HORN
RADIATOR FAN
DOOR LOCKS
BUSSED INPUTS
HEADLAMP SW
PRND STATUS
ENGINE SPEED
EGN SW STATUS
RKE COMPLEX FUNCTION REQ
TRANSM TYPE
ESP FLASH REQ
CONFIG FEATURE SPECIFIC SETTING
CONFIG FEATURE
CONFIG FEATURE STATUS REQ
SUPPRESS EXTERIOR LIGHTING
TPM HORN CHIRP REQUEST
HORN REQUEST
FRONT WASHER REQUEST
ACTIVATE PTC RELAY #3
RAD FAN #1 DUTY CYCLE
T-CASE SHIFT INHIBITED
FRONT WIPER SW
KEY IN IGNITION
RIGHT TURN SIGNAL REQ
PARK BRAKE W ENGAGED
FRONT FOG REQ
ACTIVATE PTC RELAY #1
LEFT TURN SIGNAL REQ
ELECTRIC BACKLITE REQ
RAD FAN #2 DUTY CYCLE
CHARGING SYSTEM FAILURE
ACTIVATE PTC RELAY #2
RAIN SENSOR WIPER REQ
REAR WASHER REQUEST
REAR WIPER SW
HIGH BEAM STEADY STATUS REQ
HFM SPAD REQ
DDM SPAD REQ
PANIC MODE ACTIVE
FRONT WIPER MIST REQ
PDM SPAD REQ
OPTICAL HORN REQ
AXLE LOCK SW STATUS
INVERTER ON
INVERTER REQ
VEHICLE SPEED
DRIVER CENTRAL LOCKING UNLOCK SW PRESSED
DRIVER CENTRAL LOCKING LOCK SW PRESSED
PASSENGER CENTRAL LOCKING UNLOCK SW PRESSED
PASSENGER CENTRAL LOCKING LOCK SW PRESSED
LEFT POWER SLIDING DOOR UNLOCK REQUEST
RIGHT POWER SLIDING DOOR UNLOCK REQUEST
HEADLAMP LEVEL REQUEST
AUTO HEADLAMP ON REQUEST